**AL-BAHA DOMESTIC AIRPORT (ABT) – S24 CAPACITY DECLARATION**

**Runway**

Open - 0500 UTC to 2055 UTC

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **R60 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0500-2000 | 6 | 6 | **12** |

 |

|  |
| --- |
| **R10 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0500-2000 | 1 | 1 | **0** |

 |

**Terminal**

Domestic

|  |
| --- |
| **T60/15 Terminal Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure |
| 0500-2000 | 266 | 207 |
| Load Factor: 90% |

**Check-in**

6 counters. Domestic flights open 120 minutes before STD, closes 45 minutes before STD.

2 counters per Domestic flight.

**Apron Parking**

|  |
| --- |
| **Apron** |
| **ICAO aircraft size** | Options |
| Code C | 5 |
| Code E | 1 |
| **Total** | 6 |

**Miscellaneous**

ICAO Code D and E aircraft to be referred to airport by ACL.

Separation of 30 minutes for every flight.

GABA slot requests are managed by airport directly.