**ABHA INTERNATIONAL AIRPORT (AHB) – S24 CAPACITY DECLARATION**

**Runway**

Open H24

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **R60 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 10 | 10 | **20** | | |  |  |  |  | | --- | --- | --- | --- | | **R15 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 4 | 4 | **8** | |

**Terminal Ground Service Equipment**

|  |  |
| --- | --- |
| **Pax step** | 13 |
| **ASU** | 4 |
| **GPU** | 8 |
| **ACU** | 6 |
| **Push-Back** | 8 |
| **Baggage Tractor** | 9 |
| **Conveyor Belt** | 11 |
| **HI-Loader** | 3 |
| **Water Truck** | 1 |

Domestic

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 600 | 600 |
| Load Factor: 90% | | |

**I**nternational

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 180 | 180 |
| Load Factor: 90% | | |

**Check-in**

12 counters. International flights open 180 minutes before STD, closes 60 minutes before STD. Domestic widebody flights open 165 minutes before STD, closes 45 minutes before STD. Domestic narrowbody flights open 135 minutes before STD, closes 45 minutes before STD.

International flights 3 counters per narrowbody. Domestic flights 2 counters per widebody and 1 counter per narrowbody.

1 counter reserved for Saudia Business and 1 counter reserved for Flynas.

**Gates**

4 Gates for domestic, 2 Gates for International. Maximum of 4 Gates utilised in a rolling hour.

**Apron Parking**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **Apron 1** | | | | | **ICAO aircraft size** | Options | Options | Options | | Code C | 7 | 3 | 2 | | Code E | - | 4 | 5 | | **Total** | 7 | 7 | 7 | | |  |  | | --- | --- | | **Apron 2** | | | **ICAO aircraft size** | Options | | Code C | 6 | | Code E | - | | **Total** | 6 | |

**Miscellaneous**

ICAO Code F aircraft are not permitted to operate.

Separation of 15 minutes must be applied for every departure Domestic flight. Separation of 120 minutes for every arrival International flight.

GABA slot requests are managed by airport directly.