**ARAR DOMESTIC AIRPORT (RAE) – S24 CAPACITY DECLARATION**

**Runway**

Open - 0300 UTC to 1900 UTC

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **R60 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0300-1900 | 5 | 5 | **10** | | |  |  |  |  | | --- | --- | --- | --- | | **R10 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0300-1900 | 1 | 1 | **2** | |

**Terminal**

Domestic

|  |  |  |
| --- | --- | --- |
| **T60 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0300-1900 | 220 | 220 |
| Load Factor: 90% | | |

**Check-in**

12 counters. Domestic narrowbody flights open 135 minutes before STD, closes 45 minutes before STD.

5 counters per narrowbody Domestic flight.

**Apron Parking**

|  |  |
| --- | --- |
| **Apron** | |
| **ICAO aircraft size** | Options |
| Code C | 4 |
| Code E | 2 |
| **Total** | 6 |

**Miscellaneous**

GABA slot requests are managed by airport directly.