**TURAIF DOMESTIC AIRPORT (TUI) – S24 CAPACITY DECLARATION**

**Runway**

Open - 0500 UTC to 2055 UTC

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **R60 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0500-2055 | 7 | 7 | **14** |

 |

|  |
| --- |
| **R10 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0500-2055 | 1 | 1 | **0** |

 |

**Terminal**

Domestic

|  |
| --- |
| **T60/15 Terminal Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure |
| 0500-2055 | 180 | 180 |
| Load Factor: 90% |

**Check-in**

4 counters. Domestic narrowbody flights open 135 minutes before STD, closes 45 minutes before STD.

2 counters per narrowbody Domestic flight.

**Apron Parking**

|  |
| --- |
| **Apron** |
| **ICAO aircraft size** | Options |
| Code C | 4 |
| Code D | 0 |
| **Total** | 4 |

**Miscellaneous**

GABA slot requests are managed by airport directly.