**BISHA DOMESTIC AIRPORT (BHH) – S24 CAPACITY DECLARATION**

**Runway**

Open - 0500 UTC to 2055 UTC

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **R60 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0500-2000 | 5 | 5 | **10** |

 |

|  |
| --- |
| **R15 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0500-2000 | X | X | **X** |

 |

**Terminal**

Domestic

|  |
| --- |
| **T60/15 Terminal Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure |
| 0500-2000 | 470 | 470 |
| Load Factor: 90% |

**Check-in**

8 counters. Domestic flights open 180 minutes before STD, closes 60 minutes before STD. Domestic flights 3 counters.

**Apron Parking**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **Apron** |
| **ICAO aircraft size** | Options |
| Code C | 2 |
| Code D | 1 |
| **Total** | 3 |

 |  |

**Miscellaneous**

GABA slot requests are managed by airport directly.