**BISHA DOMESTIC AIRPORT (BHH) – S24 CAPACITY DECLARATION**

**Runway**

Open - 0500 UTC to 2055 UTC

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **R60 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0500-2000 | 5 | 5 | **10** | | |  |  |  |  | | --- | --- | --- | --- | | **R15 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0500-2000 | X | X | **X** | |

**Terminal**

Domestic

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0500-2000 | 470 | 470 |
| Load Factor: 90% | | |

**Check-in**

8 counters. Domestic flights open 180 minutes before STD, closes 60 minutes before STD. Domestic flights 3 counters.

**Apron Parking**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | | **Apron** | | | **ICAO aircraft size** | Options | | Code C | 2 | | Code D | 1 | | **Total** | 3 | |  |

**Miscellaneous**

GABA slot requests are managed by airport directly.