**NAJRAN REGIONAL AIRPORT (EAM) – S24 CAPACITY DECLARATION**

**Runway**

Open – 24 Hours

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **R60 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 24 Hrs | 2 | 2 | **4** | | |  |  |  |  | | --- | --- | --- | --- | | **R15 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | X | X | X | **x** | |

**Terminal**

Domestic

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 24 Hrs | 360 | 360 |
| Load Factor: 90% | | |

International

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 24 Hrs | 180 | 180 |
| Load Factor: 90% | | |

**Check-in**

12 counters. International flights open 180 minutes before STD, closes 60 minutes before STD. Domestic narrowbody flights open 135 minutes before STD, closes 45 minutes before STD.

International flights 2 counters per narrowbody. Domestic flights 2 counter per narrowbody.

**Apron Parking**

|  |  |
| --- | --- |
| **Apron** | |
| **ICAO aircraft size** | Options |
| Code C | 8 |
| **Total** | 8 |

**Miscellaneous**

GABA slot requests are managed by airport directly.