**NEOM BAY AIRPORT (NUM) – S24 CAPACITY DECLARATION**

**Runway**

Open H24

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **R60 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0000-2300 | 5 | 5 | **10** |

 |

|  |
| --- |
| **R10 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0000-2300 | 1 | 1 | **0** |

 |

**Terminal**

Domestic

|  |
| --- |
| **T60/15 Terminal Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 450 | 450 |
| Load Factor: 90% |

**Check-in**

6 counters.

Domestic narrowbody flights open 180 minutes before STD, closes 60 minutes before STD.

Domestic Widebody flights open 180 minutes before STD, closes 60 minutes before STD.

International flights open 180 minutes before STD, closes 60 minutes before STD.

2 counters per narrowbody Domestic flight.

4 counters per Widebody Domestic flight.

2 counters per narrowbody international flight.

**Apron Parking**

|  |
| --- |
| **Apron** |
| **ICAO aircraft size** | Options |
| Code E | 6 |
| **Total** | 6 |

**Miscellaneous**

GABA slot requests are managed by airport directly.

Separation Requirements:

Between domestic and international flights (Arrival/Arrival) or (Departure/Departure) (minimum 4 hours)\*.

Between domestic wide body/ domestic wide body flights STD (minimum 2 hours).

Between domestic narrow body/ domestic wide body  flights STD (minimum 1 hour).

\*If there is an aircraft arriving from Riyadh (domestic arrival) and departing to Dubai (International departure), or

If there is an aircraft arriving from Dubai (International arrival) and departing to Riyadh (domestic departure),

This condition does not apply.

If we have two different aircraft arriving to NEOM:

* 1st aircraft from Jeddah
* 2nd aircraft form Dubai

If we have two different aircraft departing NEOM:

* 1st aircraft to Jeddah
* 2nd aircraft to Dubai

This condition applies.