**SHARUAH DOMESTIC AIRPORT (SHW) – S24 CAPACITY DECLARATION**

**Runway**

Open - 0400 UTC to 2000 UTC

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **R30 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0400-0200 | 1 | 1 | **2** |

 |

|  |
| --- |
| **R15 Slot Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure | **Total** |
| 0400-1900 | X | X | **X** |

 |

**Terminal**

Domestic

|  |
| --- |
| **T60/15 Terminal Capacity Limit** |
| **Hours (UTC)** | Arrival | Departure |
| 0400-1900 | 360 | 360 |
| Load Factor: x% |

**Check-in**

4 counters. Domestic flights open 135 minutes before STD, closes 60 minutes before STD. Domestic flights 2 counters.

**Apron Parking**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| **Apron** |
| **ICAO aircraft size** | Options |
| Code C | 3 |
| **Total** | 3 |

 |  |

**Miscellaneous**

Separation of 60 minutes for every flight.

GABA slot requests are managed by airport directly.

