**TABUK – PRINCE SULTAN BIN ADBULAZIZ AIRPORT (TUU) – S24 CAPACITY DECLARATION**

**Runway**

Open H24

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **R30 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 4 | 4 | **8** | | |  |  |  |  | | --- | --- | --- | --- | | **R15 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 2 | 2 | **X** | |

**Terminal**

Domestic

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 660 | 660 |
| Load Factor: 90% | | |

International

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 180 | 180 |
| Load Factor: 90% | | |

**Check-in**

14 counters. International flights open 180 minutes before STD, closes 60 minutes before STD. Domestic widebody flights open 135 minutes before STD, closes 45 minutes before STD. Domestic narrowbody flights open 135 minutes before STD, closes 45 minutes before STD.

4 counters per widebody International flight. 3 counters per widebody International flight. 4 counters per widebody Domestic flight. 3 counters per narrowbody Domestic flight.

**Apron Parking**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | | **Apron 1** | | | **ICAO aircraft size** | Options | | Code E | 4 | | Code C | 5 | | **Total** | 9 | |  |

**Miscellaneous**

- Separation of 60 minutes for every International flight.

-No domestic flight arrive within 30 minutes before the international flight departure due to space limitation at the arrival gates.

-GABA slot requests are managed by airport directly.