**AL-QASSIM – PRINCE NAIF BIN ABDULAZIZ INTERNATIONAL AIRPORT (ELQ) – W24 CAPACITY DECLARATION**

**Runway**

Open H24

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **R60 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 6 | 6 | **12** | | |  |  |  |  | | --- | --- | --- | --- | | **R10 Slot Capacity Limit** | | | | | **Hours (UTC)** | Arrival | Departure | **Total** | | 0000-2300 | 1 | 1 | **2** | |

**Terminal**

Domestic

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 360 | 360 |
| Load Factor: 100% | | |

International

|  |  |  |
| --- | --- | --- |
| **T60/15 Terminal Capacity Limit** | | |
| **Hours (UTC)** | Arrival | Departure |
| 0000-2300 | 180 | 180 |
| Load Factor: 100% | | |

**Check-in**

8 international counters & 9 domestic counters. International flights open 180 minutes before STD, closes 60 minutes before STD. Domestic widebody flights open 165 minutes before STD, closes 45 minutes before STD. Domestic narrowbody flights open 165 minutes before STD, closes 45 minutes before STD.

3 counters per International flight. 3 counters per widebody Domestic flight. 2 counters per narrowbody Domestic flight.

**Apron Parking**

|  |  |
| --- | --- |
| **Apron** | |
| **ICAO aircraft size** | Options |
| Code C | 12 |
| Code E | 1 |
| **Total** | 13 |

**Miscellaneous**

ICAO Code D and E aircraft to be referred to airport by ACL.

GABA slot requests are managed by airport directly.

Separation of 30 minutes must be applied between arriving & departing Domestic flights.

Separation of 60 minutes must be applied between arriving & departing International flights.